|  |  |  |  |
| --- | --- | --- | --- |
| **2020-2021** |  |  | **PART I** |
|  | **State Price Quote Specification****TYPE D60—BID AS 48 PASSENGER****Use this document to bid both non-lift and lift buses for 35–60 capacity.** |  Vendor:SCHETKY NW SALES, INC.  |
|  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the state cost. |
| Seating Capacity | 48 passenger based upon an average center-to-center seat spacing of at least 27.5”. | Capacity w/o lift 48  |
| Capacity w/lift 34  |
| Alternator | 240 amp minimum. Lift-equipped or air-conditioned. Manufacturer recommended capacity. | Mfr. LEECE-NEVILLE  |
| Amps output w/o lift or A.C. 240  |
| Amps output w/lift or A.C. 240  |
| Auxiliary Fans | 2 fans, 6” maximum, mounted to right and left windshield and service door. | Mfr. BERGSTROM  |
| Axle—Front | 10,000 lb. minimum. | Mfr. DETROIT  |
| Capacity 13,200LBS  |
| Axle—Rear | 19,000 lb. minimum. | Mfr. DETROIT  |
| Capacity 19,000LBS  |
| Axle Oil Seals | Front and rear oil bath. | Mfr. CHICAGO RAWHIDE  |
| Axle Ratio | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications Manual. | Ratio 5.71  |
| Back-up Lights | All required backup lights to be LED (Light Emitting Diode). Refer to Washington State School Bus Specification’s Manual. | Round: [ ]  Diameter 7" Other: [x]  Square inches 22"  |
| Battery(ies) | 1200 CCA 12 volt minimum to be mounted in body battery compartment w/o lift. | Size/group w/o lift 31 CCA 1520  |
| 1400 CCA 12 volt minimum to be mounted in body battery compartment w/lift.  | Size/group w/lift 31 CCA 1520  |
| Battery Compartment | Battery storage tray must be large enough to accommodate batteries as specified in chassis section. | [ ]  Swing out | [x]  Roll out |
| Brakes | Hydraulic disc. Refer to Washington State School Bus Specifications Manual. | Size Front 15" X 1.44" Rear 15" X 1.44"  |

PART I (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification****TYPE D60—BID AS 48 PASSENGER****Use this document to bid both non-lift and lift buses for 35–60 capacity.** |  Vendor:SCHETKY NW SALES, INC.  |
|  |
|  |  |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the state cost. |
| Door, Service | Power operated. | [x]  Air[ ]  Electric[ ]  Other | [ ]  Folding[x]  Split, Outward opening[ ]  Other |
| Engine | Diesel—180 H.P. minimum. | Engine mfr. CUMMINS  |
| Model or liters ISB 200  |
| Net torque 520 @ 1600 R.P.M  |
| Net H.P. 200 @ 2400 R.P.M  |
| Location: Rear [ ]  Forward [x]  |
| Engine Heater | Engine manufacturer’s recommended in-block heater. | Watts 750  | Volts 120  |
| Mfr. KIM  |
| Engine Temperature | To be controlled electronically, by fan clutch/drive, or shutters. | Mfr. THOMAS  |  [x]  Electronic |
| [ ]  Fan clutch |  [ ]  Shutters |
| Fuel Tank | 60 gallon minimum. | Capacity 60 GAL  |
| Heaters | Minimum of 3 heaters; 1 front, 1 center, 1 rear. Shutoff valves at engine for all heaters. Two-speed motors. Must include recirculating pump. | Front B.T.U. 90,000  |
| Center B.T.U. 50,000  |
| Rear B.T.U. 50,000  |
| Total B.T.U. 190,000  |
| Lights | LED (Light Emitting Diode). Includes Clearance Lights, Stop Lights–7”, Tail Lights, Turn Signals, Eight-Light System, and Dome-Light System. | Check if as specified [x] If not, explain   |
| P.A. System | AM/FM/PA radio with 2 interior and 1 exterior speakers. | Mfr. PANASONIC  |
| Model No. B260101301 INC. CD PLAYER  |
| Seat Spacing | To permit specified passenger capacity based on an average center-to-center seat spacing of at least 27.5”. | Inside measurement from rear of stepwell toappropriate point at rear of passengerseating area: w/o lift 316.8 w/lift 316.8  |
| Mfg.’s C/C seat measurement of vehicle(inches): w/o lift 30.3 w/lift 30.3  |

PART I (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification****TYPE D60—BID AS 48 PASSENGER****Use this document to bid both non-lift and lift buses for 35–60 capacity.** |  Vendor:SCHETKY NW SALES, INC.  |
|  |
|  |  |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the state cost. |
| Steering Wheel | Tilt and telescoping column. | Check if as specified [x]  |
| Step Tread | Studded or pebbled top tread covering. | Mfr. RCA  |
| Tires | 6 first quality, radial ply. No low profile tires. | Mfr. HANKOOK  |
| Size 11R22.5  |
| Load range G  |
| Toolbox | Exterior, manufacturer standard. | Size (cubic feet) 3.37  |
| Transmission | Automatic—Allison, PTS 2500 or equal. | Mfr. ALLISON  |
| Model no. PTS 2500  |
| Net input torque 550 GROSS  |
| Net input H.P. 300GROSS  |
| Two-way Communications | 45-watt, VHF, mil. spec. | Mfr. KENWOOD  |
| Model No. TK-7302HVK 50 WATTS VHF  |
| Wheels | 6 to be compatible with tire size. | Size 22.5  |
| Rim width 7.5  |

PART I (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification****TYPE D60—BID AS 48 PASSENGER****Use this document to bid both non-lift and lift buses for 35–60 capacity.** |  Vendor:SCHETKY NW SALES, INC.  |
|  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the state cost. |
|  | **SPECIAL NEEDS REQUIREMENTS—CHASSIS AND BODY** |  |
| WheelchairLift—Installed | Must meet state specification. Platform shall be a minimum of 32” x 52”. | Mfr. BRAUN  |
| Model No. NCL919FIB-2  |
| Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | Mfr. SURE-LOK  |
| Model No. FF627S-4C-3  |
|  | **ADDITIONAL REQUIREMENTS—CHASSIS AND BODY** |  |
| Line Setting Ticket | Legible copy of manufacturer’s Line Setting Ticket will be delivered with each vendor’s packet at the time of delivery of the bus. | Check if as specified [x]  |
| Owner’s/Operator’s Handbook | One copy of the chassis manufacturer’s owner’s/operator’s handbook or manual will be furnished with each bus at time of delivery. | Check if as specified [x]  |
| Repair Manuals | A complete set of chassis, engine, transmission, and body repair manuals, including wiring diagram for all components, will be made available at time of delivery, with instructions available on accessing repair materials. | Check if as specified [x]  |
| Service and Cleaning | Cleaning and service by vendor prior to delivery will include:* Chassis lubrication.
* Check fluid levels: verify all are at recommended full levels.
* Cooling system protected at -20°F.
* Interior and exterior will be clean (including glass).
* All systems (electric, air, hydraulic, mechanical and manual) be inspected to ensure proper operation at time of delivery.
* All components and accessories will be installed and operational at time of delivery.
 | Check if as specified [x]  |
| Warranty | A complete copy of all warranty agreements will be furnished at time of delivery. | Check if as specified [x]  |

|  |  |
| --- | --- |
| **2020-2021** |  STUDENT TRANSPORTATION Old Capitol Building PO BOX 47200 Olympia, WA 98504-7200 (360) 725-6120 TTY (360) 664-3631 **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION** **TYPE D60—BID AS 48 PASSENGER** |
|  |  |
| VENDOR’S COMPANY NAMESCHETKY NW SALES, INC.  | REPRESENTATIVE’S NAMEKIM HEVIA | TELEPHONE NUMBER503-382-3126 |
| ADDRESS8430 NE KILLINGSWORTH ST. PORTLAND, OR. 97220 | Estimated delivery date to school district from time purchase order is received: 180-220 DAYS ARO Firm where engine and chassis can beserviced or repaired and parts obtained: ANY AUTHORIZED CUMMINS OR THOMAS DEALER Firm where body can be serviced or repaired and parts obtained: SCHETKY NW SALES, INC.  |
|  |

|  |
| --- |
| **BODY** |
| MAKETHOMAS BUILT BUSES  | Warranty: Years 1-5 Miles UNLTDSeat color: GRAYFloor color: BLACK | Inside measurement from rear of stepwell to appropriate point at rear of passenger seating area: w/o lift 287" w/lift 287"  | Equipped seating capacity: w/o lift 48 w/lift 37 Overall vehicle length (inches): w/o lift 337.8 w/lift 337.8  |
| MODEL0918S | YEAR2021/2022 |

|  |  |
| --- | --- |
| **CHASSIS** | **ENGINE** |
| MAKETHOMAS BUILT BUSES | Warranty: Years 1-5 Miles UNLTD | MANUFACTURERCUMMINS | Torque: 520 @ 1600 RPMH.P.: 200 @ 2400 RPM |
| MODEL0918S | YEAR2021/2022 | Wheel base: 136 " | MODELISB 200 | YEARNEW | C.I.D. or Liters: 6.7LFuel type: DIESEL |
| **TRANSMISSION** | Warranty: Years 5  Miles 100KNumber of cylinders: 6Inline X V-type       | Battery type/grp: 31 31Number batteries: 2 2Total CCA: 1520 1520 |
| MANUFACTURERALLISON | Speeds forward: 5 |
| MODELPTS 2500 | Warranty: Years 7 Miles UNLTD |

|  |
| --- |
| **QUOTED PRICE** |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).Bid—w/o lift $ 101,329.00 Bid—w/lift $ 104,539.00  |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

PART II

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification****DISTRICT-SUPPORTED OPTIONS****[ ]  C60** **[ ]  C77** **[x]  D60** **[ ]  D84****Use this document to bid both non-lift and lift buses.** |  Vendor:SCHETKY NW SALES, INC.  |
|  |
|  |  |  |
| **ITEM** | Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Activity Securement Seating | 2-passenger position seats with lap-shoulder belts in all passenger positions. | Passenger Capacity 32  |
| Cost $ 950.00 PER SEAT  |
| Air Conditioning | To cool passenger compartment as required in the Washington State School Bus Specifications manual. | Mfr. CARRIER  |
| Cost $ 10,292.00 104K BTU SYSTEM  |
| Alternate Fuel | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications manual. Must comply with all of the requirements of FMVSS No. 305. | Mfr. N/A  |
| [ ]  CNG | [ ]  CNG Cost $ N/A  |
| [ ]  Electric | [ ]  Electric Cost $ N/A  |
| Alternator | Available options. | Cost $ 985.00 Capacity 270  |
| Cost $ 995.00 Capacity 275  |
| Cost $ 1,400.00 Capacity 320  |
| Anti-spray Device | Rubber fender extenders. | Type C: Cost $        |
| Type D: Cost $ 350.00 (4)  |
| Back-up Alarm | Must meet state specification. | Mfr. THOMAS  |
| Cost $ 115.00  |
| Brakes | 4-wheel hydraulic disk brake. | Cost $ INC.  | Deduct $ N/A  |
| Brakes | Air, Drum or Disc. Refer to Washington State School Bus Specifications manual. | Disc Cost $ 4,350.00  | Disc Deduct $ N/A  |
| Drum Cost $ 3,650.00  | Drum Deduct $ N/A  |
| Color | Exterior white roof. | Cost $ 695.00  |
| Door Locks | Vandal lock system on all exterior doors. | Cost $ 325.00  |
| Driver’s Seat | Suspension type, 6-way adjustable, with lumbar adjustment. Cloth panel covers. | ***Non-Air*** | ***Air*** |
| Mfr. NATIONAL  | Mfr. NATIONAL  |
| Cost $ INCLUDED  | Cost $ 525.00  |
| Fire Suppression System | Jomarr VT-6-E-NAF, or equal engine compartment fire suppression system of appropriate size to be installed according to manufacturer recommendation. | Mfr. FOG MAKER  |
| Cost $ 4,100.00  |
| Floor Color | Nonstandard color. | Cost $ 870.00 GRAY  |

PART II (cont.)

|  |
| --- |
| Vendor:SCHETKY NW SALES, INC. **State Price Quote Specification****DISTRICT-SUPPORTED OPTIONS** **[ ]  C60 [ ]  C77 [x]  D60 [ ]  D84****Use this document to bid both non-lift and lift buses.** |
|  |  |  |
| **ITEM** | Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Fuel Tank | Larger fuel capacity (CNG only). | Size: N/A  | Cost $ N/A  |
| Fuel Tank | Larger fuel capacity (Diesel only). | Size: N/A  | Cost $ N/A  |
| Fuel Tank | Larger fuel capacity (Propane only). | Size: N/A  | Cost $ N/A  |
| Headlights | Halogen. | Cost $ INCLUDED  |
| Headlights | L.E.D. | Cost $ 650.00 FACTORY INSTALLED  |
| Heater (Auxiliary water) | Auxiliary fuel-fired heating systems. Refer to Washington State School Bus Specifications Manual, page 27. | Brand: WEBASTO Model: 45K BTU  |
| Cost $ 4,400.00 RS ONLY  |
| Noise Reduction | Exceeding minimum specifications. | Driver compartment Cost $ 250.00  |
| Engine compartment Cost $ 310.00  |
| Full acoustical headliner Cost $ 750.00  |
| Retarder | Manufacturer’s standard. | Driveline [ ]  Cost $ N/A  |
| Exhaust [x]  Cost $ 150.00  |
| Transmission [ ]  Cost $ N/A  |
| Seat Belt Ready Seat | 3-passenger position seat with belts. | Cost $ 1,025.00 PER SEAT  |
| Seating System | Identical, non-lift bus with lap-shoulder seat belt system installed in all positions. | 2 by 2 Cost $ 7,525.00  |
| Capacity 32  |
| 3 by 2 Cost $ 7,450.00  |
| Capacity 40  |
| 3 by 3 Cost $ 8,100.00  |
| Capacity 48  |

PART II (cont.)

|  |
| --- |
| Vendor:SCHETKY NW SALES, INC. **State Price Quote Specification****DISTRICT-SUPPORTED OPTIONS** **[ ]  C60 [ ]  C77 [x]  D60 [ ]  D84****Use this document to bid both non-lift and lift buses.** |
|  |  |  |
| **ITEM** | Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Storage Compartments | Largest available for unit bid. | Left-side N/A cubic feet. |
| Cost $ N/A  |
| Right-side 15.5 cubic feet. |
| Cost $ 1,250.00  |
| Push-thru N/A cubic feet. |
| Cost $ N/A  |
| Strobe Light | Exterior roof mounted white strobe light. | Mfr. THOMAS  |
| Model No. DOUBLE FLASH  |
| Cost $ 230.00  |
| Student Protection System—Installed | Electronic system to insure driver post-trip inspection of passenger compartment. | Mfr. THOMAS  |
| Model No. B200104000  |
| Cost $ 330.00  |
| Suspension | Air ride (Air brake system only). | ***Front*** | ***Rear*** |
| Cost $ N/A  | Cost $ 4,025.00  |
| Toolbox | Interior, manufacturer standard. | Cost $ 55.00  | Deduct $ N/A  |
| Traction Device | Automatic chains. | Mfr. ON SPOT  |
| Cost $ 3,075.00  |
| Traction Device | Sanders. | Capacity 158 LBS  |
| Cost $ 3,700.00  |
| Transmission | Automatic—Allison, PTS 3000 or equal. | Mfr. ALLISON  |
| Model No. 3000PTS  |
| Cost $ 5,875.00  |
| Vehicle Securement System | Must meet state specification. | Mfr. SAFETY BRAKE  | Cost $ 1,150.00  |

PART II (cont.)

|  |
| --- |
| Vendor:Schetky NW Sales Inc **State Price Quote Specification****DISTRICT-SUPPORTED OPTIONS** **[ ]  C60 [ ]  C77 [x]  D60 [ ]  D84****Use this document to bid both non-lift and lift buses.** |
|  |  |  |
| **ITEM** | Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Video Camera Systems—Installed | Digital audio/video system for monitoring the passenger compartment with more than two cameras. | Mfr. AMERICAN BUS VIDEO  |
| Model No. RSD4MX-4  |
| Cost $ 2,350.00 How many cameras 4 |
| Video Camera Systems—Stop Sign Camera—Installed | Must meet state specification. | ***Stand Alone System*** | ***Added to Interior System*** |
| Mfr. AMERICAN BUS VIDEO  | Mfr. AMERICAN BUS VIDEO  |
| Model No. RSD4HD-1  | Model No. SACA 12MM  |
| Cost $ 1,550.00  | Cost $ 450.00  |
| How many cameras 1 | How many cameras 1 |
| Warning Light Monitor | 16 light monitoring system. | ***Incandescent*** | ***LED Lights*** |
| Cost $ 275.00  | Cost $ 780.00  |
| Additional Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | Mfr. SURE-LOK  |
| Model No. FF627S-4C-3  |
| Cost per station $ 895.00 WITH FLOOR POCKETS  |
| Windows | Laminated passenger-compartment side or rear glass. | Side Cost $ 1,500.00  |
| Rear Cost $ INC WITH SIDE WINDOWS  |
| Both Cost $ 1,500.00  |
| Windows | Tinted. | Cost $ 425.00  |
| Windows | Thermal pane, left of driver and service door. | Cost $ 895.00  |