|  |  |  |  |
| --- | --- | --- | --- |
| **2022-2023** |  |  | **PART I** |
|  | **State Price Quote Specification****TYPE D—84 PASSENGER, REAR ENGINE****Use this document to bid both non-lift and lift buses for 61 – 84 capacity.** |  Vendor:  |
|   |
|  |  |  |
| **ITEM** | **SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Seating Capacity | 84 passenger maximum design capacity seated for 78 passenger. | Capacity w/o lift  |
| Capacity w/lift  |
| Alternator | 240 amp minimum. Lift-equipped or air-conditioned. Manufacturer recommended capacity. | Mfr.  |
| Amps output w/o lift or A.C. Amps output w/lift or A.C.  |
| Auxiliary Fans | 2 fans, 6” maximum, mounted to right and left windshield and service door. | Mfr.  |
| Axle—Front | 13,200 lb. minimum total suspension GVWR. | Mfr.  |
| Capacity  |
| Axle—Rear | 23,000 lb. minimum total suspension GVWR. | Mfr.  |
| Capacity  |
| Axle Oil Seals | Front and rear oil bath. | Mfr.  |
| Axle Ratio | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications Manual. | Ratio  |
| Back-up Lights | All required backup lights to be LED (Light Emitting Diode). Refer to Washington State School Bus Specification’s Manual. | Round: [ ]  Diameter Other: [ ]  Square inches  |
| Battery(ies) | 1400 CCA 12 volt to be mounted in body battery compartment.  | Number of batteries  |
| CCA  |
| Battery Compartment | Battery storage tray must be large enough to accommodate batteries as specified in chassis section. | [ ]  Swing out [ ]  Roll out |
| Brakes | Air: Drum or Disc. If Drum, minimum 16.5” x 6” front, minimum 16.5” x 8” rear. Refer to Washington State School Bus Specifications Manual. | Disc Front [ ]  Rear [ ]  |
| Drum Front [ ]  Rear [ ]  |
| Size Front Rear df  |
| Door, Service | Power operated. | [ ]  Folding [ ]  Other[ ]  Roll out |
| [ ]  Split, Outward opening |
| Driver’s Seat | Suspension type, 6-way adjustable, with lumbar adjustment. Cloth panel covers. | Mfr.  |

PART I (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification****TYPE D—84 PASSENGER, REAR ENGINE****Use this document to bid both non-lift and lift buses for 61 – 84 capacity.** |  Vendor:        |
|         |
|  |  |  |
| **ITEM** | **SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Engine | Diesel—280 H.P. minimum, located in the rear. | Engine mfr.        |
| Model or liters        |
| Net torque       @       R.P.M  |
| Net H.P.       @       R.P.M  |
| Engine Heater | Engine manufacturer’s recommended in-block heater. | Watts        | Volts        |
| Mfr.        |
| Engine Temperature | To be controlled electronically, by fan clutch/drive, or shutters. | Mfr.        |  [ ]  Electronic |
| [ ]  Fan clutch |  [ ]  Shutters |
| Fuel Tank | 100 gallon minimum. | Capacity        |
| Heaters | Minimum of 3 heaters; 1 front, 1 center, 1 rear. Shutoff valves at engine for all heaters. Two-speed motors. Must include recirculating pump. | Front B.T.U.        |
| Center B.T.U.        |
| Rear B.T.U.        |
| Total B.T.U.        |
| Lights | LED (Light Emitting Diode). Includes Clearance Lights, Stop Lights–7”, Tail Lights, Turn Signals, Eight-Light System, and Dome-Light System. | Check if as specified [ ] If not, explain   |
| P.A. System | AM/FM/PA radio with 4 interior and 1 exterior speakers. | Mfr.        |
| Model No.        |
| Seat Spacing | 78 passenger based upon manufacturer’s maximum seat spacing. | Inside measurement from rear of stepwell to appropriate point at rear of passenger seating area:       inches |
| Mfg.’s C/C seat measurement:       inches  |
| Steering Wheel | Tilt and telescoping column. | Check if as specified [ ]  |
| Step Tread | Studded or pebbled top tread covering. | Mfr.        |
| Tires | 6 first quality, radial ply. No low profile tires. | Mfr.        |
| Size        |
| Load range        |

PART I (cont.)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | **State Price Quote Specification****TYPE D—84 PASSENGER, REAR ENGINE** |  Vendor:               |  |
|  |  |

**Use this document to bid both non-lift and lift buses for 61 – 84 capacity.**

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | **SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Toolbox | Exterior, manufacturer standard. | Size (cubic feet)        |
| Transmission | Automatic—Allison, PTS 3000 or equal. | Mfr.        |
| Model no.        |
| Net input torque        |
| Net input H.P.        |
| Two-way Communications | 45-watt, VHF, mil. spec. | Mfr.        |
| Model No.        |
| Wheels | 6 to be compatible with tire size. | Size        |
| Rim width        |
|  | **SPECIAL NEEDS REQUIREMENTS—CHASSIS AND BODY** |  |
| WheelchairLift—Installed | Must meet state specification. Platform shall be a minimum of 32” x 52”. | Mfr.        |
| Model No.        |
| Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | Mfr.        |
| Model No.        |

PART I (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification****TYPE D—84 PASSENGER, REAR ENGINE****Use this document to bid both non-lift and lift buses for 61 – 84 capacity.** |  Vendor:        |
|         |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | **SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
|  | **ADDITIONAL REQUIREMENTS—CHASSIS AND BODY** |  |
| Line Setting Ticket | Legible copy of manufacturer’s Line Setting Ticket will be delivered with each vendor’s packet at the time of delivery of the bus. | Check if as specified [ ]  |
| Owner’s/Operator’s Handbook | One copy of the chassis manufacturer’s owner’s/operator’s handbook or manual will be furnished with each bus at time of delivery. | Check if as specified [ ]  |
| Repair Manuals | A complete set of chassis, engine, transmission, and body repair manuals, including wiring diagram for all components, will be made available at time of delivery, with instructions available on accessing repair materials. | Check if as specified [ ]  |
| Service and Cleaning | Cleaning and service by vendor prior to delivery will include:* Chassis lubrication.
* Check fluid levels: verify all are at recommended full levels.
* Cooling system protected at -20°F.
* Interior and exterior will be clean (including glass).
* All systems (electric, air, hydraulic, mechanical and manual) be inspected to ensure proper operation at time of delivery.
* All components and accessories will be installed and operational at time of delivery.
 | Check if as specified [ ]  |
| Warranty | A complete copy of all warranty agreements will be furnished at time of delivery. | Check if as specified [ ]  |

|  |  |
| --- | --- |
| **2022-2023** |  STUDENT TRANSPORTATION Old Capitol Building PO BOX 47200 Olympia, WA 98504-7200 (360) 725-6120 TTY (360) 664-3631 **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION** **TYPE D—84 PASSENGER, REAR ENGINE** |
|  |  |
| VENDOR’S COMPANY NAME      | REPRESENTATIVE’S NAME      | TELEPHONE NUMBER      |
| ADDRESS      | Estimated delivery date to school district from time purchase order is received:       Firm where engine and chassis can be serviced or repaired and parts obtained:        Firm where body can be serviced or repaired and parts obtained:        |
|  |

|  |
| --- |
| **BODY** |
| MAKE      | Warranty: Years       Miles      Seat color:      Floor color:       | Inside measurement from rear of stepwell to appropriate point at rear of passenger seating area: w/o lift       w/lift        | Equipped seating capacity: w/o lift       w/lift       Overall vehicle length (inches): w/o lift       w/lift        |
| MODEL      | YEAR      |

|  |  |
| --- | --- |
| **CHASSIS** | **ENGINE** |
| MAKE      | Warranty: Years       Miles       | MANUFACTURER      | Torque:       @       RPMH.P.:       @       RPM |
| MODEL      | YEAR      | Wheel base:       | MODEL      | YEAR      | C.I.D.:      Fuel type:       |
| **TRANSMISSION** | Warranty: Years        Miles      Number of cylinders:      Inline       V-type       | Battery type/grp:            Number batteries:            Total CCA:             |
| MANUFACTURER      | Speeds forward:       |
| MODEL      | Warranty: Years       Miles       |

|  |
| --- |
| **QUOTED PRICE** |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).Bid—w/o lift $       Bid—w/lift $        |
| VENDOR REPRESENTATIVE’S SIGNATURE      | DATE      |

PART II

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification****DISTRICT-SUPPORTED OPTIONS**[ ]  **C60** [ ]  **C77** [ ]  **D60** [ ]  **D84****Use this document to bid both non-lift and lift buses.** | Vendor:        |
|        |
|  |  |  |
| **ITEM** | Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Activity Securement Seating | 2-passenger position seats with lap-shoulder belts in all passenger positions. | Passenger Capacity        |
| Cost $        |
| Air Conditioning | To cool passenger compartment as required in the Washington State School Bus Specifications manual. | Mfr.        |
| Cost $        |
| Alternate Fuel | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications manual. Must comply with all of the requirements of FMVSS No. 305. | Mfr.        |
| [ ]  CNG | [ ]  CNG Cost $        |
| [ ]  Electric | [ ]  Electric Cost $        |
| Alternator | Available options. | Cost $       Capacity        |
| Cost $       Capacity        |
| Cost $       Capacity        |
| Anti-spray Device | Rubber fender extenders. | Type C: Cost $        |
| Type D: Cost $        |
| Back-up Alarm | Must meet state specification. | Mfr.        |
| Cost $        |
| Brakes | 4-wheel hydraulic disk brake. | Cost $        | Deduct $        |
| Brakes | Air, Drum or Disc. Refer to Washington State School Bus Specifications manual. | Disc Cost $        | Disc Deduct $        |
| Drum Cost $        | Drum Deduct $        |
| Color | Exterior white roof. | Cost $        |
| Door Locks | Vandal lock system on all exterior doors. | Cost $        |
| Driver’s Seat | Suspension type, 6-way adjustable, with lumbar adjustment. Cloth panel covers. | ***Non-Air*** | ***Air*** |
| Mfr.        | Mfr.        |
| Cost $        | Cost $        |
| Fire Suppression System | Jomarr VT-6-E-NAF, or equal engine compartment fire suppression system of appropriate size to be installed according to manufacturer recommendation. | Mfr.        |
| Cost $        |
| Floor Color | Nonstandard color. | Cost $        |

PART II (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification****DISTRICT-SUPPORTED OPTIONS**[ ]  **C60** [ ]  **C77** [ ]  **D60** [ ]  **D84****Use this document to bid both non-lift and lift buses.** | Vendor:        |
|        |
|  |  |  |
| **ITEM** | Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Fuel Tank | Larger fuel capacity (CNG only). | Size:        | Cost $        |
| Fuel Tank | Larger fuel capacity (Diesel only). | Size:        | Cost $        |
| Fuel Tank | Larger fuel capacity (Propane only). | Size:        | Cost $        |
| Headlights | Halogen. | Cost $        |
| Headlights | L.E.D. | Cost $        |
| Heater (Auxiliary water) | Auxiliary fuel-fired heating systems. Refer to Washington State School Bus Specifications Manual, page 27. | Brand:       Model:        |
| Cost $        |
| Noise Reduction | Exceeding minimum specifications. | Driver compartment Cost $        |
| Engine compartment Cost $        |
| Full acoustical headliner Cost $        |
| Retarder | Manufacturer’s standard. | Driveline [ ]  Cost $        |
| Exhaust [ ]  Cost $        |
| Transmission [ ]  Cost $        |
| Seat Belt Ready Seat | 3-passenger position seat with securement belts. | Cost $        |
| Seating System | Identical, non-lift bus with lap-shoulder seat belt system installed in all positions. | 2 by 2 Cost $        |
| Capacity        |
| 3 by 2 Cost $        |
| Capacity        |
| 3 by 3 Cost $        |
| Capacity        |

PART II (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification****DISTRICT-SUPPORTED OPTIONS**[ ]  **C60** [ ]  **C77** [ ]  **D60** [ ]  **D84****Use this document to bid both non-lift and lift buses.** | Vendor:        |
|        |
|  |  |  |
| **ITEM** | Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Storage Compartments | Largest available for unit bid. | Left-side       cubic feet. |
| Cost $        |
| Right-side       cubic feet. |
| Cost $        |
| Push-thru       cubic feet. |
| Cost $        |
| Strobe Light | Exterior roof mounted white strobe light. | Mfr.        |
| Model No.        |
| Cost $        |
| Student Protection System—Installed | Electronic system to insure driver post-trip inspection of passenger compartment. | Mfr.        |
| Model No.        |
| Cost $        |
| Suspension | Air ride (Air brake system only). | ***Front*** | ***Rear*** |
| Cost $        | Cost $        |
| Toolbox | Interior, manufacturer standard. | Cost $        | Deduct $        |
| Traction Device | Automatic chains. | Mfr.        |
| Cost $        |
| Traction Device | Sanders. | Capacity        |
| Cost $        |
| Transmission | Automatic—Allison, PTS 3000 or equal. | Mfr.        |
| Model No.        |
| Cost $        |
| Vehicle Securement System | Must meet state specification. | Mfr.        | Cost $        |

PART II (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification****DISTRICT-SUPPORTED OPTIONS**[ ]  **C60** [ ]  **C77** [ ]  **D60** [ ]  **D84****Use this document to bid both non-lift and lift buses.** | Vendor:        |
|        |
|  |  |  |
| **ITEM** | Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Video Camera Systems—Installed | Digital audio/video system for monitoring the passenger compartment with more than two cameras. | Mfr.        |
| Model No.        |
| Cost $       How many cameras       |
| Video Camera Systems—Stop Sign Camera—Installed | Must meet state specification. | ***Stand Alone System*** | ***Added to Interior System*** |
| Mfr.        | Mfr.        |
| Model No.        | Model No.        |
| Cost $        | Cost $        |
| How many cameras       | How many cameras       |
| Warning Light Monitor | 16 light monitoring system. | ***Incandescent*** | ***LED Lights*** |
| Cost $        | Cost $        |
| Additional Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | Mfr.        |
| Model No.        |
| Cost per station $        |
| Windows | Laminated passenger-compartment side or rear glass. | Side Cost $        |
| Rear Cost $        |
| Both Cost $        |
| Windows | Tinted. | Cost $        |
| Windows | Thermal pane, left of driver and service door. | Cost $        |