|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo**2017-18** |  |  | **PART I** |
|  | **State Price Quote Specification****TYPE A— DIESEL, GAS & PROPANE****Use this document to bid both non-lift and lift, gas, diesel and propane buses.** |  Vendor: Creative Bus Sales  Mfr.: Starcraft  |
|  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the state cost. |
| Seating Capacity | Maximum passenger capacity based upon an average center-to-center seat spacing of at least 27.5” with a lap-shoulder belt for each seating position. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Capacity w/o lift 25  | Capacity w/o lift 22  | Capacity w/o lift 23  |
| Capacity w/lift 18+1WC  | Capacity w/lift 16+1WC  | Capacity w/lift 18+1WC  |
| Alternator | 145 amp minimum. Lift-equipped or air-conditioned. Manufacturer recommended capacity. | Mfr. Ford  |
| Amps output w/o lift or A.C. 145  |
| Amps output w/lift or A.C. 145  |
| Auxiliary Automatic Transmission Cooler | 10,000 lb. Hayden or equal. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Mfr. Ford  | Mfr. Ford  | Mfr. Ford  |
| Lbs. rating 10,360  | Lbs. rating 10,360  | Lbs. rating 12500  |
| Axle—Front | Manufacturer’s recommendation. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Mfr. Ford  | Mfr. Ford  | Mfr. Ford  |
| Capacity 4130  | Lbs. rating 4130  | Lbs. rating 5000  |
|  |  | Indepen. suspens. [ ]  | Indepen. suspens. [ ]  | Indepen. suspens. [ ]  |
| Axle—Rear | Manufacturer’s recommendation. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Mfr. Ford  | Mfr. Ford  | Mfr. Ford  |
| Capacity 7275  | Capacity 7275  | Capacity 7800  |
| Axle Ratio | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications Manual. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Ratio 3.73  | Ratio 3.73  | Ratio 4.10  |
| Back-up Lights | All required backup lights to be LED (Light Emitting Diode). Refer to Washington State School Bus Specification’s Manual. | Round: [x]  Diameter 4" Other: [ ]  Square inches        |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification****TYPE A— DIESEL, GAS & PROPANE****Use this document to bid both non-lift and lift, gas, diesel and propane buses.** |  Vendor: Creative Bus Sales  Mfr.: Starcraft  |
|  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the state cost. |
| Battery(ies) | 535 CCA 12 volt minimum for gas and propane w/o lift.1070 CCA 12 volt minimum for diesel or any bus w/lift. | ***Gas/Propane w/o lift*** | ***Diesel or any bus w/lift*** |
| CCA 600  | CCA 1540  |
| Brakes | Hydraulic: Drum or Disc. Refer to Washington State School Bus Specifications Manual. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Front Disc [x]  | Front Disc [x]  | Front Disc [x]  |
|  Drum [ ]  |  Drum [ ]  |  Drum [ ]  |
| Rear Disc [x]  | Rear Disc [x]  | Rear Disc [x]  |
|  Drum [ ]  |  Drum [ ]  |  Drum [ ]  |
| Drum Size        | Drum Size        | Drum Size        |
| Doors, Service | Power operated. | [ ]  Air [x]  Folding [x]  Electric[ ]  Split, Outward Opening [ ]  Other        |
| Engine | Gas and Propane—3.7 liters minimum.Diesel—130 H.P. minimum. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Engine mfr. Ford  | Engine mfr. Ford  | Engine mfr. Ford  |
| Liters 3.7L  | H.P. 190  | Liters 6.8L  |
| Engine Heater | Diesel only—engine manufacturer’s recommended in-block heater. | Watts 400  | Volts 110AC  |
| Mfr. OEM  |
| Fuel Tank | Gas and Diesel—25 gallon minimum.Propane—largest available. | ***Gas/Diesel*** | ***Propane*** |
| Capacity 25  | Capacity 35  |
| Hand Throttle | Diesel only—locking type, electronic, or immediate acting electric fast idle. |  [ ]  Vernier |  [x]  Electric |
|  [ ]  T type |  [ ]  Electronic |
| Heaters | Front—manufacturer’s standard. Rear—40,000 B.T.U. minimum. | Rear B.T.U. w/o lift 65K Rear B.T.U. w/lift 65K  |
| Lights | LED (Light Emitting Diode). Includes Clearance Lights, Stop Lights–7”, Tail Lights, Turn Signals, Eight-Light System, and Dome-Light System. | Check if as specified [x] If not, explain   |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification****TYPE A— DIESEL, GAS & PROPANE****Use this document to bid both non-lift and lift, gas, diesel and propane buses.** |  Vendor: Creative Bus Sales  Mfr.: Starcraft  |
|  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the state cost. |
| P.A. System | AM/FM/PA radio with 2 interior and 1 exterior speakers. | Mfr. Jensen  |
| Model No. JBR550/PA500  |
| Seat Spacing | To permit specified passenger capacity based on an average center-to-center seat spacing of at least 27.5”. | Inside measurement from rear of stepwell toappropriate point at rear of passenger seatingarea: w/o lift 160.1875 w/lift 160.1875  |
| Mfg.’s C/C seat measurement ofvehicle (inches): w/o lift 27.5" w/lift 27.5"  |
| Steering Wheel | Tilt. | Check if as specified [x]  |
| Step Tread | Studded or pebbled top tread covering. | Mfr. Koroseal  |
| Tires | 6 first quality, radial ply.  | Mfr. OEM  |
| Size LT195/75x16C, LT225/75x16E  |
| Load range E  |
| Toolbox | Exterior, manufacturer standard. | Size (cubic feet) 3.35  |
| Transmission | Automatic—manufacturer’s standard compatible with H.P. and torque rating of engine bid. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Mfr. Ford  | Mfr. Ford  | Mfr. Ford  |
| Model no. 6R80  | Model no. 6R80  | Model no. 6R140  |
| Two-way Communications | 45-watt, VHF, mil. spec. | Mfr. ICOM  |
| Model No. F5011 Series  |
| Wheels | 6 to be compatible with tire size. | Size 16  |
| Rim width 6.5  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification****TYPE A— DIESEL, GAS & PROPANE****Use this document to bid both non-lift and lift, gas, diesel and propane buses.** |  Vendor: Creative Bus Sales  Mfr.: Starcraft  |
|  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the state cost. |
|  | **SPECIAL NEEDS REQUIREMENTS—CHASSIS AND BODY** |  |
| WheelchairLift—Installed | Must meet state specification. Platform shall be a minimum of 32” x 52”. | Mfr. Braun  |
| Model No. Century NCL919IB-2  |
| Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | Mfr. Q-Straint  |
| Model No. Q8101/Q8-6326-A1  |
|  | **ADDITIONAL REQUIREMENTS—CHASSIS AND BODY** |  |
| Line Setting Ticket | Legible copy of manufacturer’s Line Setting Ticket will be delivered with each vendor’s packet at the time of delivery. | Check if as specified [x]  |
| Owner’s/Operator’s Handbook | One copy of the chassis manufacturer’s owner’s/operator’s handbook or manual will be furnished with each bus at delivery. | Check if as specified [x]  |
| RFID Tag | WSP school bus inspection identification tag. | Check if as specified [x]  |
| Repair Manuals | A complete set of chassis, engine, transmission, and body repair manuals, including wiring diagram for all components, will be made available at time of delivery, with instructions available on accessing repair materials. | Check if as specified [x]  |
| Service and Cleaning | Cleaning and service by vendor prior to delivery will include:* Chassis lubrication.
* Check fluid levels: verify all are at recommended full levels.
* Cooling system protected at -20°F.
* Interior and exterior will be clean (including glass).
* All systems (electric, air, hydraulic, mechanical and manual) be inspected to ensure proper operation at time of delivery.
* All components and accessories will be installed and operational at time of delivery.
 | Check if as specified [x]  |
| Warranty | A complete copy of all warranty agreements will be furnished at time of delivery. | Check if as specified [x]  |

|  |  |
| --- | --- |
| OSPI Logo**2017-18** |  STUDENT TRANSPORTATION Old Capitol Building PO BOX 47200 Olympia, WA 98504-7200 (360) 725-6120 TTY (360) 664-3631 **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION** **TYPE A—DIESEL** |
|  |  |
| VENDOR’S COMPANY NAMECREATIVE BUS SALES | REPRESENTATIVE’S NAMELONNIE SOLMONSON | TELEPHONE NUMBER360-515-1801 |
| ADDRESS11601 CYRUS WAYMUKILTEO, WA. 98275 | Estimated delivery date to school district from time purchase order is received: 150-180 DAYS Firm where engine and chassis can beserviced or repaired and parts obtained: ANY FORD COMMERCIAL DEALER Firm where body can be serviced or repaired and parts obtained: CREATIVE BUS SALES, MUKILTEO WA.  |
|  |

|  |
| --- |
| **BODY** |
| MAKESTARCRAFT | Warranty: Years 3 Miles 36,000Seat color: GRAYFloor color: BLACK | Inside measurement from rear of stepwell to appropriate point at rear of passenger seating area: w/o lift 187.5" w/lift 187.5"  | Equipped seating capacity: w/o lift 22 w/lift 16 Overall vehicle length (inches): w/o lift 294" w/lift 294"  |
| MODELQUEST | YEAR2018 |

|  |  |
| --- | --- |
| **CHASSIS** | **ENGINE** |
| MAKESTARCRAFT | Warranty: Years 3 Miles 36,000 | MANUFACTURERFORD | Torque: 350 @ 1500 RPMH.P.: 185 @ 2500 RPM |
| MODELTRANSIT | YEAR2018 | Wheel base: 156 | MODEL3.2L I5 DIESEL | YEAR2018 | Fuel type: DIESEL |
| **TRANSMISSION** | Warranty: Years 5  Miles 60,000Number of cylinders: 5Inline x V-type       | Battery type/grp: 72AH 72AHNumber batteries: 2 2Total CCA: 1540 1540 |
| MANUFACTURERFORD | Speeds forward: 6 |
| MODEL6R80 | Warranty: Years 5 Miles 60,000 |

|  |
| --- |
| **QUOTED PRICE** |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).Diesel Bid—w/o lift $ 59596.00 Diesel Bid—w/lift $ 63811.00  |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |
| --- | --- |
| OSPI Logo**2017-18** |  STUDENT TRANSPORTATION Old Capitol Building PO BOX 47200 Olympia, WA 98504-7200 (360) 725-6120 TTY (360) 664-3631 **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION** **TYPE A—GAS** |
|  |  |
| VENDOR’S COMPANY NAMECREATIVE BUS SALES | REPRESENTATIVE’S NAMELONNIE SOLMONSON | TELEPHONE NUMBER360-515-1801 |
| ADDRESS11601 CYRUS WAYMUKILTEO, WA 98275 | Estimated delivery date to school district from time purchase order is received: 150-180 DAYS Firm where engine and chassis can beserviced or repaired and parts obtained: ANY FORD DEALER Firm where body can be serviced or repaired and parts obtained: CREATIVE BUS SALES  |
|  |

|  |
| --- |
| **BODY** |
| MAKESTARCRAFT | Warranty: Years 3 Miles 36,000Seat color: GREYFloor color: BLACK | Inside measurement from rear of stepwell to appropriate point at rear of passenger seating area: w/o lift 187.5" w/lift 187.5"  | Equipped seating capacity: w/o lift 25 w/lift 18 Overall vehicle length (inches): w/o lift 294" w/lift 294"  |
| MODELQUEST | YEAR2018 |

|  |  |
| --- | --- |
| **CHASSIS** | **ENGINE** |
| MAKEFORD | Warranty: Years 3 Miles 36,000 | MANUFACTURERFORD | Torque: 260 @ 4000 RPMH.P.: 275 @ 6000 RPM |
| MODELTRANSIT | YEAR2018 | Wheel base: 156 | MODEL3.7L | YEAR2018 | Liters: 3.7LFuel type: GAS |
| **TRANSMISSION** | Warranty: Years 5  Miles 60,000Number of cylinders: 6Inline       V-type X | Battery type/grp: 72AH 72AHNumber batteries: 1 2Total CCA: 615 1540 |
| MANUFACTURERFORD | Speeds forward: 6 |
| MODEL6R80 | Warranty: Years 5 Miles 60,000 |

|  |
| --- |
| **QUOTED PRICE** |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).Gas Bid—w/o lift $ 55679.00 Gas Bid—w/lift $ 59064.00  |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |
| --- | --- |
| OSPI Logo**2017-18** |  STUDENT TRANSPORTATION Old Capitol Building PO BOX 47200 Olympia, WA 98504-7200 (360) 725-6120 TTY (360) 664-3631 **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION** **TYPE A—PROPANE** |
|  |  |
| VENDOR’S COMPANY NAMECREATIVE BUS SALES | REPRESENTATIVE’S NAMELONNIE | TELEPHONE NUMBER360-515-1801 |
| ADDRESS11601 CYRUS WAYMUKILTEO, WA. 98275 | Estimated delivery date to school district from time purchase order is received: 150-180 DAYS Firm where engine and chassis can beserviced or repaired and parts obtained: ANY FORD DEALER Firm where body can be serviced or repaired and parts obtained: CREATIVE BUS SALES  |
|  |

|  |
| --- |
| **BODY** |
| MAKESTARCRAFT | Warranty: Years 3 Miles 36,000Seat color: GREYFloor color: BLACK | Inside measurement from rear of stepwell to appropriate point at rear of passenger seating area: w/o lift 187" w/lift 187"  | Equipped seating capacity: w/o lift 25 w/lift 18 Overall vehicle length (inches): w/o lift 294" w/lift 294"  |
| MODELQUEST | YEAR2018 |

|  |  |
| --- | --- |
| **CHASSIS** | **ENGINE** |
| MAKEFORD | Warranty: Years 3 Miles 36,000 | MANUFACTURERFORD | Torque: 420 @ 3250 RPMH.P.: 305 @ 4250 RPM |
| MODELE350 | YEAR2018 | Wheel base: 158" | MODEL6.8L | YEAR2018 | Liters: 6.8LFuel type: GAS |
| **TRANSMISSION** | Warranty: Years 5  Miles 60,000Number of cylinders: 10Inline       V-type X | Battery type/grp: 72AH 72AHNumber batteries: 2 2Total CCA: 1350 1350 |
| MANUFACTURERFORD | Speeds forward: 6 |
| MODEL6R140 | Warranty: Years 5 Miles 60,000 |

|  |
| --- |
| **QUOTED PRICE** |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).Propane Bid—w/o lift $ 73,179.00 Propane Bid—w/lift $ 77,144.00  |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART II** |
|  | **State Price Quote Specification****DISTRICT-SUPPORTED OPTIONS****TYPE A****Use this document to bid both non-lift and lift, gas, diesel and propane buses.** |  Vendor: CREATIVE BUS SALES  Mfr.: STARCRAFT  |
|  |

|  |  |  |
| --- | --- | --- |
|  | **CHASSIS** |  |
| **ITEM** | Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Small A | Type A bus—10,000 lbs or under GVWR chassis. | ***Gas*** |  ***Diesel***  | ***Propane*** |
| Deduct $1,000.00  | Deduct $1,000.00  | Deduct N/A  |
| Mfr. STARCRAFT  | Mfr. STARCRAFT  | Mfr. N/A  |
| Capacity w/o lift 16  | Capacity w/o lift 14  | Capacity w/o lift N/A  |
| Dual Wheel [ ]  | Dual Wheel [ ]  | Dual Wheel [ ]  |
| Single Wheel [x]  | Single Wheel [x]  | Single Wheel [ ]  |
| Air Conditioning | To cool passenger compartment as required in the Washington State School Bus Specifications manual. | Mfr. TRANSAIR  |
| Cost $ 1525.00  |
| Alternate Fuel | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications manual. | Mfr. N/A  |
| [ ]  CNG | [ ]  CNG Cost $ N/A  |
| [ ]  Other | [ ]  Other Cost $ N/A  |
| Back-up Alarm | Must meet state specification. | Mfr. ECCO  |
| Cost $ 25.00  |
| Color | Exterior white roof. | Cost $ STANDARD  |
| Steering Wheel | Tilt and telescoping column. | Cost $ TILT ONLY  |
| Strobe Light | Exterior roof mounted white strobe light. | Mfr. SOUND OFF SIGNAL  |
| Model No. 3107LCC  |
| Cost $ 185.00  |
| Student Protection System—Installed | Electronic system to insure driver post-trip inspection of passenger compartment.  | Mfr. CHILD CHECKMATE  |
| Model No. DLRH-1  |
| Cost $ 175.00  |
| Toolbox | Interior, manufacturer standard. | Cost $ 190.00  | Deduct $ $100.00  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART II (cont.)** |
|  | **State Price Quote Specification****DISTRICT-SUPPORTED OPTIONS****TYPE A****Use this document to bid both non-lift and lift, gas, diesel and propane buses.** |  Vendor: CREATIVE BUS SALES  Mfr.: STARCRAFT  |
|  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Video Camera Systems—Installed | Digital audio/video system for monitoring the passenger compartment with more than two cameras. | Mfr. SAFETY VISION  |
| Model No. 4000HYB-128GKI  |
| Cost $ 2202.00 How many cameras 3 |
| Video Camera Systems—Stop Sign Camera—Installed | Must meet state specification. | ***Stand Alone System*** | ***Added to Interior System*** |
| Mfr. SAFETY VISION  | Mfr. SAFETY VISION  |
| Model No. 4000HYB-128  | Model No. 4000HYB-128  |
| Cost $ 1606.00  | Cost $ 2379.00  |
| How many cameras 1 | How many cameras 4 |
| Warning Light Monitor | 16 light monitoring system. | ***Incandescent*** | ***LED Lights*** |
| Cost $ 400.00  | Cost $ 400.00  |
| Additional Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | Mfr. Q-STRAINT  |
| Model No. Q8101/Q8-6326-A1  |
| Cost per station $ 1,050.00  |
| Windows | Laminated passenger-compartment side or rear glass. | Side Cost $ 840.00  |
| Rear Cost $ 450.00  |
| Both Cost $ 1,300.00  |
| Windows | Tinted. | Cost $ STANDARD  |